PAGE  
[image: image1.jpg]


KIOXIA LIGHT RING EQUIPMENT GROUP CO.,LTD.
[image: image6.png]WWWWWWWWWWWWWW



  TEL/WhatsApp: +86 17622605414
Mail: admin@transformercoilwindingmachine.com
    Web:www.transformercoilwindingmachine.com

NAME：KX-9800 Transformer Parallel Winding Machine
[image: image7.png]o«
2
2

‘ \®
KIOXIA
LIGHT RING





SPECIFICATION:
	Spindles
	1
	Spread Motor
	stepping Motor

	Wire diameter
	0.08-0.8mm
	Max Speed
	6000rpm

	Spread Pitch
	0-9.999mm
	Memory
	999 Sequences

	Spread Width
	100mm（Max）
	Power Source
	AC 220V/110V±10%,50/60MHZ

	Winding Width
	200mm（Max）
	Weight
	37 KG

	Main Motor
	1/8HP DC Motor
	Dimension
	76×68×72cm


FEATURES:

1.Transformer Parallel Winding Machine has microprocessor design ,easy for program-setting handing.

2.Wire guiding traverse shaft stepper motor with a constant-current driver offering fast wire guiding speed.

Multiple spindles synchronal winding for highest efficiency

3.More convenience by using foot-switch

4.Transformer Parallel Winding Machine is specially designed for winding toroidal / rectangular /oval cores from CRGO electrical silicon steel full automatically.

5.Transformer Parallel Winding Machine adtops Panasonic PLC control system, full closed-loop control all the procedure, including clamping, fixing, pressing, winding, cutting, welding, releasing, etc.

ADVANTAGES:

1.You can change the program to achieve functionality as needed.
2.The position of the spool can be adjust with the teaching function, which can assist the setting of the winding point and width position.
3.0~999 group data is easy to set, with powerful DC motor and precision stepper motor, it can easily set forward reverse, cross slot and flow tight winding work.
4.Transformer Parallel Winding Machine can be equipped with lengthened winding width, the longest wire width can be arranged 1500mm
5.Winding head adopt guide pin, winding wire will be  neat and accurate
6.Wire wheel adopts ceramic guide wheel, high temperature resistance and non - damage enameled wire.

APPLICATION:

Typical applications for high torsion parallel spindle winding Machine with a single wire size, include the manufacture of gas ignition coils, solenoids, relays, motors and many forms of sensor coil in small and medium batch quantities.It is ideal for use in the production of small inductors, particularly bobbins wound with a single wire size and high turns count. The high maximum winding spindle speed (up to 6000 rpm) enables coils with a high turns count to be wound in a short cycle time.
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PRACTICAL APPLICATION :

Training for Customers to Operate KX-9800 Transformer Parallel Winding Machine

1.All service engineers with 10 years of experience have received special technical training, including specialized expertise in the KX-9800 Transformer Parallel Winding Machine, enabling them to effectively handle various breakdown issues specific to this parallel-winding equipment, such as multi-axis synchronization failures, parallel coil tension mismatches, or program errors in simultaneous winding sequences.

2.We guide users to accurately operate and maintain the KX-9800 Transformer Parallel Winding Machine—with focused attention to its parallel winding parameter configuration, multi-coil synchronization setup, wire tension balancing across channels, and maintenance of key components like parallel spindle drives and coordinate control systems—while providing free consultation about the production process technology related to electronic transformer manufacturing, including optimal parallel winding strategies for efficiency and consistency.

3.To ensure the KX-9800 Transformer Parallel Winding Machine operates normally, we conduct dedicated training on its parallel winding operational protocols, program customization for different transformer types, and preventive maintenance of multi-axis systems through English manuals, model-specific instructional videos, and real-time online guidance—all tailored to the unique parallel-winding capabilities of this transformer production equipment.
PACKAGING:

Packaging Material: Carton/Wooden case with foam inside.
1.General package(Paper carton or plastic bag): For small euipped parts for Transformer Parallel Winding Machine, Package it with form and pack paper to guarantee unbroken during the transport.
2.Wooden case package: For larger scale Transformer Parallel Winding Machine,we have special skilled carpenter, who would make the proper wooden case with exact thickness,density,length. The up arrow ↑marked on the outer wooden case. Buffer material would be put in the wooden case to prevent crack and shock.
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OPTIONAL ACCESSORIES

	NO.
	Item/Specification
	QUANTITY
	UNIT

	1 
	controller
	1
	PIECE

	2 
	winding motor
	1
	PIECE

	3 
	Spread motor
	1
	PIECE

	4 
	optical fiber sensor
	1
	PIECE

	5 
	B2-2.0 Inches shuttle
	1
	PIECE

	6 
	4 inches and 6 inches shuttle                                                           (base on machine model)
	1
	PIECE

	7 
	shuttle guide wheel
	1
	PIECE

	8 
	fixture head
	1
	PIECE

	9 
	green round belt                                                                                 (can send one free in orange)
	1
	M

	10 
	gear shape belt
	1
	Belt


FACTORY:

We, KIOXIA LIGHT RING EQUIPMENT GROUP CO.,LTD., have been experts in winding machine lines for 28 years, with our advanced product range featuring specialized equipment like the KX-9800 Transformer Parallel Winding Machine—a cutting-edge system engineered for efficient parallel winding of transformer coils, embodying our technical innovation in high-productivity transformer manufacturing solutions.

Our KIOXIA LIGHT RING brand holds authoritative certifications and recognitions, including ISO9001:2015, CE approvals, multiple machine patents (encompassing key innovations in parallel winding technology for models like the KX-9800 Transformer Parallel Winding Machine), and the official designation of "high-tech enterprise" by the government. These credentials validate the reliability, precision, and efficiency of our entire product portfolio, reinforcing our commitment to delivering superior winding solutions for diverse transformer production needs.
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KIOXIA LIGHT RING EQUIPMENT GROUP CO.,LTD.
Add: Building G, No.209 Zhonghuan East Road, Free Trade Zone (Airport Economic Zone), Tianjin

